IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Numéro du projet"
Time stamp: "2019-06-16T16:49:15"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190225_1515(x64) - Exporter 19.1.0.0 - Interface alternative d'export 19.1.0.0"
Application: "Autodesk Revit 2019 (FRA)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (FRA)"

People and organizations
  Person "Serge" "Doroginsky" of Organization (no name given)
  Owner history of Person "Serge" "Doroginsky" of Organization (no name given) | application "Autodesk Revit 2019 (FRA)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (FRA)" | change NOCHANGE | created 1560693449 (2019-06-16T13:57:29Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Numéro du projet" | phase "PRO"
IFCROOF "Toit de base:tuile terre cuite:5220084" | object type "Toit de base:tuile terre cuite"
  IFCSLAB "Toit de base:tuile terre cuite:5220084" | object type "Toit de base:tuile terre cuite" | ROOF
  IFCSLAB "Toit de base:tuile terre cuite:5220084" | object type "Toit de base:tuile terre cuite" | ROOF
  IFCSLAB "Toit de base:tuile terre cuite:5220084" | object type "Toit de base:tuile terre cuite" | ROOF
  IFCSLAB "Toit de base:tuile terre cuite:5220084" | object type "Toit de base:tuile terre cuite" | ROOF
IFCROOF "Toit de base:tuile terre cuite:5220622" | object type "Toit de base:tuile terre cuite"
  IFCSLAB "Toit de base:tuile terre cuite:5220622" | object type "Toit de base:tuile terre cuite" | ROOF
  IFCSLAB "Toit de base:tuile terre cuite:5220622" | object type "Toit de base:tuile terre cuite" | ROOF
  IFCSLAB "Toit de base:tuile terre cuite:5220622" | object type "Toit de base:tuile terre cuite" | ROOF
  IFCSLAB "Toit de base:tuile terre cuite:5220622" | object type "Toit de base:tuile terre cuite" | ROOF
IFCBUILDINGSTOREY "N 00" | long name "N 00" | object type "Niveau:Ligne du Niveau" | elevation 151.3052
  contains 599 elements
    15 x IFCWALLSTANDARDCASE | object type "Mur de base:Bard bois vertical + MOB + contre cloison BA18" | names: "Mur de base:Bard bois vertical + MOB + contre cloison BA18:5005861", "Mur de base:Bard bois vertical + MOB + contre cloison BA18:5005871", "Mur de base:Bard bois vertical + MOB + contre cloison BA18:5005876" (+12 more) | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
    38 x IFCWALLSTANDARDCASE | object type "Mur de base:Refend MOB 16 cm+ contre cloison BA18" | names: "Mur de base:Refend MOB 16 cm+ contre cloison BA18:5005862", "Mur de base:Refend MOB 16 cm+ contre cloison BA18:5005874", "Mur de base:Refend MOB 16 cm+ contre cloison BA18:5005887" (+35 more) | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    19 x IFCWALLSTANDARDCASE | object type "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18" | names: "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18:5005866", "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18:5005867", "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18:5005872" (+16 more) | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    2 x IFCWALL | object type "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18" | names: "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18:5005870", "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18:5176814" | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    106 x IFCWALLSTANDARDCASE | object type "Mur de base:84/48 BA18 isol 45" | names: "Mur de base:84/48 BA18 isol 45:5005895", "Mur de base:84/48 BA18 isol 45:5005904", "Mur de base:84/48 BA18 isol 45:5005905" (+103 more) | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    7 x IFCWALLSTANDARDCASE | object type "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18" | names: "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18:5028041", "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18:5176817", "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18:5176818" (+4 more) | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
    16 x IFCDOOR | object type "POR Double:183x204cm" | names: "POR Double:183x204cm:5031922", "POR Double:183x204cm:5031966", "POR Double:183x204cm:5032200" (+13 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    34 x IFCWALLSTANDARDCASE | object type "Mur de base:Séparation sanitaires 3/6" | names: "Mur de base:Séparation sanitaires 3/6:5034099", "Mur de base:Séparation sanitaires 3/6:5035777", "Mur de base:Séparation sanitaires 3/6:5035778" (+31 more) | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    16 x IFCWALLSTANDARDCASE | object type "Mur de base:Cloison mobile à galandage" | names: "Mur de base:Cloison mobile à galandage:5040160", "Mur de base:Cloison mobile à galandage:5040483", "Mur de base:Cloison mobile à galandage:5040539" (+13 more) | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
    3 x IFCDOOR | object type "Va et vient double - Double Oculus rond:1.83m x 2.04m - (180)" | names: "Va et vient double - Double Oculus rond:1.83m x 2.04m - (180):5053748", "Va et vient double - Double Oculus rond:1.83m x 2.04m - (180):5053815", "Va et vient double - Double Oculus rond:1.83m x 2.04m - (180):5055751" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    32 x IFCDOOR | object type "POR Simple:92x204" | names: "POR Simple:92x204:5054333", "POR Simple:92x204:5057713", "POR Simple:92x204:5058188" (+29 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    4 x IFCWALL | object type "Mur de base:84/48 BA18 isol 45" | names: "Mur de base:84/48 BA18 isol 45:5055704", "Mur de base:84/48 BA18 isol 45:5358542", "Mur de base:84/48 BA18 isol 45:5358685" (+1 more) | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    22 x IFCDOOR | object type "POR-1V-VITREE:205x105" | names: "POR-1V-VITREE:205x105:5055946", "POR-1V-VITREE:205x105:5056081", "POR-1V-VITREE:205x105:5056137" (+19 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    7 x IFCDOOR | object type "POR-2V-DOUBLE-VITREE:205x210" | names: "POR-2V-DOUBLE-VITREE:205x210:5057196", "POR-2V-DOUBLE-VITREE:205x210:5102415", "POR-2V-DOUBLE-VITREE:205x210:5104083" (+4 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    7 x IFCDOOR | object type "POR Simple:82x204" | names: "POR Simple:82x204:5060529", "POR Simple:82x204:5060576", "POR Simple:82x204:5060603" (+4 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    5 x IFCDOOR | object type "POR Double:143x229cm" | names: "POR Double:143x229cm:5061053", "POR Double:143x229cm:5092204", "POR Double:143x229cm:5293298" (+2 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    3 x IFCDOOR | object type "porte metallique ADS.0001:1.83m x 2.04m" | names: "porte metallique ADS.0001:1.83m x 2.04m:5061306", "porte metallique ADS.0001:1.83m x 2.04m:5096211", "porte metallique ADS.0001:1.83m x 2.04m:5197519" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    3 x IFCDOOR | object type "porte metallique ADS.0001:1.43m x 2.04m" | names: "porte metallique ADS.0001:1.43m x 2.04m:5061340", "porte metallique ADS.0001:1.43m x 2.04m:5176908", "porte metallique ADS.0001:1.43m x 2.04m:5176944" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCSLAB | object type "Sol:Linoleum_Veneto_Silencio_xf2_Apple Green_14892754" | FLOOR | names: "Sol:Linoleum_Veneto_Silencio_xf2_Apple Green_14892754:5070436" | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes
    10 x IFCWINDOW | object type "Fenêtre ronde:D 600 mm" | names: "Fenêtre ronde:D 600 mm:5090273", "Fenêtre ronde:D 600 mm:5090573", "Fenêtre ronde:D 600 mm:5090620" (+7 more) | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCSTAIR | object type "Escalier coulé sur place:Monobloc" | names: "Escalier coulé sur place:Escalier:5091198" | property sets: Pset_QuantityTakeOff, Pset_StairCommon, Autre, Contraintes, Cotes, Données d'identification
    11 x IFCCOVERING | object type "Plafond composé:Faux plafond type ecophon hygiène 600x600" | CEILING | names: "Plafond composé:Faux plafond type ecophon hygiène 600x600:5095652", "Plafond composé:Faux plafond type ecophon hygiène 600x600:5095660", "Plafond composé:Faux plafond type ecophon hygiène 600x600:5095684" (+8 more) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCDOOR | object type "porte metallique ADS.0001:Alu 1.83m x 2.04m" | names: "porte metallique ADS.0001:Alu 1.83m x 2.04m:5103349" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    12 x IFCWINDOW | object type "FEN-METAL-COULISSANT-DOUBLE:h160x240 Triple Vitrage- Store intérieur- 1 ouvrant OB et 2 fixes" | names: "FEN-METAL-COULISSANT-DOUBLE:h160x240 Triple Vitrage- Store intérieur- 1 ouvrant OB et 2 fixes:5106042", "FEN-METAL-COULISSANT-DOUBLE:h160x240 Triple Vitrage- Store intérieur- 1 ouvrant OB et 2 fixes:5106151", "FEN-METAL-COULISSANT-DOUBLE:h160x240 Triple Vitrage- Store intérieur- 1 ouvrant OB et 2 fixes:5107267" (+9 more) | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    4 x IFCWINDOW | object type "FEN-METAL-COULISSANT-DOUBLE:160x240 Store Griesser aluminium 1 ouvrant OB et 2 fixes" | names: "FEN-METAL-COULISSANT-DOUBLE:160x240 Store Griesser aluminium 1 ouvrant OB et 2 fixes:5106360", "FEN-METAL-COULISSANT-DOUBLE:160x240 Store Griesser aluminium 1 ouvrant OB et 2 fixes:5109239", "FEN-METAL-COULISSANT-DOUBLE:160x240 Store Griesser aluminium 1 ouvrant OB et 2 fixes:5109279" (+1 more) | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    15 x IFCWINDOW | object type "FEN-METAL-COULISSANT-DOUBLE:Chassis h1.60 x 240 aluminium 1 ouvrant OB et 2 fixes" | names: "FEN-METAL-COULISSANT-DOUBLE:Chassis h1.60 x 240 aluminium 1 ouvrant OB et 2 fixes:5106693", "FEN-METAL-COULISSANT-DOUBLE:Chassis h1.60 x 240 aluminium 1 ouvrant OB et 2 fixes:5108488", "FEN-METAL-COULISSANT-DOUBLE:Chassis h1.60 x 240 aluminium 1 ouvrant OB et 2 fixes:5108818" (+12 more) | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    6 x IFCWINDOW | object type "FEN-METAL-COULISSANT-DOUBLE:160x120 triple vitrage store interieur" | names: "FEN-METAL-COULISSANT-DOUBLE:160x120 triple vitrage store interieur:5108172", "FEN-METAL-COULISSANT-DOUBLE:160x120 triple vitrage store interieur:5108228", "FEN-METAL-COULISSANT-DOUBLE:160x120 triple vitrage store interieur:5108261" (+3 more) | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    3 x IFCWINDOW | object type "FEN-METAL-COULISSANT-DOUBLE:160x120 2" | names: "FEN-METAL-COULISSANT-DOUBLE:160x120 2:5110986", "FEN-METAL-COULISSANT-DOUBLE:160x120 2:5111312", "FEN-METAL-COULISSANT-DOUBLE:160x120 2:5111536" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCDOOR | object type "Porte metallique simple1:83 x 204 cm - béquille" | names: "Porte metallique simple1:83 x 204 cm - béquille:5114830" | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    2 x IFCBEAM | object type "Poutre rectangulaire - Béton:200 x 600 mm" | names: "Poutre rectangulaire - Béton:200 x 600 mm:5176789", "Poutre rectangulaire - Béton:200 x 600 mm:5176795" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam, Autre, Contraintes, Cotes
    1 x IFCBEAM | object type "Poutre rectangulaire - Béton:coupe feu" | names: "Poutre rectangulaire - Béton:coupe feu:5176793" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam, Autre, Contraintes, Cotes
    1 x IFCBEAM | object type "Poutre rectangulaire - Béton:400 x 600 mm" | names: "Poutre rectangulaire - Béton:400 x 600 mm:5176797" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam, Autre, Contraintes, Cotes
    1 x IFCWALL | object type "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18" | names: "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18:5176810" | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
    2 x IFCCURTAINWALL | object type "Mur-rideau:Facade panneau simple" | names: "Mur-rideau:Facade panneau simple:5176867", "Mur-rideau:Facade panneau simple:5176886" | parts: 19 IFCMEMBER, 10 IFCPLATE, 2 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    2 x IFCDOOR | object type "POR-2V-DOUBLE-VITREE:205x200" | names: "POR-2V-DOUBLE-VITREE:205x200:5176925", "POR-2V-DOUBLE-VITREE:205x200:5433355" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    9 x IFCELEMENTASSEMBLY | object type "Assemblage Mobilier:table enfant ronde 6" | USERDEFINED | names: "Assemblage Mobilier:table enfant ronde 6:5176954", "Assemblage Mobilier:table enfant ronde 6:5176962", "Assemblage Mobilier:table enfant ronde 6:5176970" (+6 more) | property sets: Pset_QuantityTakeOff, Autre, Données d'identification, Phase de construction
    9 x IFCELEMENTASSEMBLY | object type "Assemblage Mobilier:Mobilier 005" | USERDEFINED | names: "Assemblage Mobilier:Mobilier 005:5177026", "Assemblage Mobilier:Mobilier 005:5177034", "Assemblage Mobilier:Mobilier 005:5177050" (+6 more) | property sets: Pset_QuantityTakeOff, Autre, Données d'identification, Phase de construction
    15 x IFCELEMENTASSEMBLY | object type "Assemblage Mobilier:table 6" | USERDEFINED | names: "Assemblage Mobilier:table 6:5177098", "Assemblage Mobilier:table 6:5177106", "Assemblage Mobilier:table 6:5177120" (+12 more) | property sets: Pset_QuantityTakeOff, Autre, Données d'identification, Phase de construction
    1 x IFCELEMENTASSEMBLY | object type "Assemblage Mobilier:Mobilier 001" | USERDEFINED | names: "Assemblage Mobilier:Mobilier 001:5177112" | property sets: Pset_QuantityTakeOff, Autre, Données d'identification, Phase de construction
    2 x IFCELEMENTASSEMBLY | object type "Assemblage Mobilier:table 4" | USERDEFINED | names: "Assemblage Mobilier:table 4:5177134", "Assemblage Mobilier:table 4:5177155" | property sets: Pset_QuantityTakeOff, Autre, Données d'identification, Phase de construction
    2 x IFCSLAB | object type "Sol:Dalle en béton 20 + iso 10" | FLOOR | names: "Sol:Dalle en béton 20 + iso 10:5177284", "Sol:Dalle en béton 20 + iso 10:5288178" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes, Cotes
    1 x IFCSLAB | object type "Sol:Finition sol souple" | FLOOR | names: "Sol:Finition sol souple:5177315" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes, Cotes
    1 x IFCSLAB | object type "Sol:Linoleum_Veneto_Silencio_xf2_Carmine_14892645" | FLOOR | names: "Sol:Linoleum_Veneto_Silencio_xf2_Carmine_14892645:5177327" | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes
    1 x IFCSLAB | object type "Sol:Finition carrelage" | FLOOR | names: "Sol:Finition carrelage:5177351" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes, Cotes
    1 x IFCSTAIR | object type "Escalier coulé sur place:Escalier technique" | names: "Escalier coulé sur place:Escalier:5177364" | property sets: Pset_QuantityTakeOff, Pset_StairCommon, Autre, Contraintes, Cotes, Phase de construction
    3 x IFCWINDOW | object type "1 Vantail - Droit:0.45m x 0.45m - Appui Alu" | names: "1 Vantail - Droit:0.45m x 0.45m - Appui Alu:5177512", "1 Vantail - Droit:0.45m x 0.45m - Appui Alu:5177513", "1 Vantail - Droit:0.45m x 0.45m - Appui Alu:5177514" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    4 x IFCWINDOW | object type "PF 2 vantaux + 2 fixés - Droits:chassis menuisé largeur 5.00x h 1.60" | names: "PF 2 vantaux + 2 fixés - Droits:chassis menuisé largeur 5.00x h 1.60:5177677", "PF 2 vantaux + 2 fixés - Droits:chassis menuisé largeur 5.00x h 1.60:5177678", "PF 2 vantaux + 2 fixés - Droits:chassis menuisé largeur 5.00x h 1.60:5177679" (+1 more) | property sets: Pset_QuantityTakeOff, Pset_WindowCommon, Autre, Contraintes, Cotes, Données d'identification
    9 x IFCWALLSTANDARDCASE | object type "Mur de base:MOB + Bardage horizontal" | names: "Mur de base:MOB + Bardage horizontal:5197099", "Mur de base:MOB + Bardage horizontal:5197103", "Mur de base:MOB + Bardage horizontal:5197195" (+6 more) | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
    4 x IFCSLAB | object type "Sol:Enrobé végétaux a froid" | FLOOR | names: "Sol:Enrobé végétaux a froid:5218786", "Sol:Enrobé végétaux a froid:5219985", "Sol:Enrobé végétaux a froid:5230787" (+1 more) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes, Cotes
    8 x IFCCOLUMN | object type "Poteau - Lamellé-collé - Pin du sud:300x300mm" | names: "Poteau - Lamellé-collé - Pin du sud:300x300mm:5219163", "Poteau - Lamellé-collé - Pin du sud:300x300mm:5219173", "Poteau - Lamellé-collé - Pin du sud:300x300mm:5219657" (+5 more) | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Autre, Contraintes, Cotes
    1 x IFCFURNISHINGELEMENT | object type "Portail_2m MC_8-6-8:3259x1105mm" | names: "Portail_2m MC_8-6-8:3259x1105mm:5258155" | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
    2 x IFCWALLSTANDARDCASE | object type "Mur de base:MOB + Bardage bois vertical" | names: "Mur de base:MOB + Bardage bois vertical:5263984", "Mur de base:MOB + Bardage bois vertical:5264082" | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    1 x IFCBUILDINGELEMENTPROXY | object type "SAFIR-007_Portail_coulissant_SAFIR_Ixxo_2-3D-T-50-100-FBLR:portail coulissant 2" | names: "SAFIR-007_Portail_coulissant_SAFIR_Ixxo_2-3D-T-50-100-FBLR:portail coulissant 2:5271456" | property sets: Pset_BuildingElementProxyCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes
    2 x IFCWALLSTANDARDCASE | object type "Mur de base:Acrotère - enduit 2 + isolant 12 + MOB + enduit" | names: "Mur de base:Acrotère - enduit 2 + isolant 12 + MOB + enduit:5286634", "Mur de base:Acrotère - enduit 2 + isolant 12 + MOB + enduit:5287175" | property sets: Autre, Contraintes, Cotes, Phase de construction, Structure, Pset_QuantityTakeOff
    2 x IFCSLAB | object type "Sol:Aire de jeux sol souple ext" | FLOOR | names: "Sol:Aire de jeux sol souple ext:5310625", "Sol:Aire de jeux sol souple ext:5313661" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes, Cotes
    2 x IFCFURNISHINGELEMENT | object type "Casier:Sloped Roof Cabinet 1861x300x400" | names: "Casier:Sloped Roof Cabinet 1861x300x400:5333031", "Casier:Sloped Roof Cabinet 1861x300x400:5333080" | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Construction, Contraintes, Cotes
    5 x IFCBUILDINGELEMENTPROXY | object type "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC" | names: "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5338266", "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5338386", "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5347860" (+2 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    4 x IFCDOOR | object type "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 4m" | names: "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 4m:5354983", "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 4m:5358435", "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 4m:5358543" (+1 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    8 x IFCDOOR | object type "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 3m80" | names: "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 3m80:5355712", "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 3m80:5355856", "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 3m80:5356177" (+5 more) | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    21 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358090", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358091", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358092" (+18 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
    1 x IFCDOOR | object type "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 3m30" | names: "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 3m30:5359911" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCDOOR | object type "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 5m20" | names: "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 5m20:5360050" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCDOOR | object type "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 2m50" | names: "Placard coulissante - 3 panneaux:Placard coulissante - 3 panneaux 2m50:5360511" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCSLAB | object type "Sol:Plancher Bois sur VS" | FLOOR | names: "Sol:Plancher Bois sur VS:5381791" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes, Cotes
    1 x IFCDOOR | object type "POR-1V-VITREE:205x100" | names: "POR-1V-VITREE:205x100:5382367" | property sets: Pset_DoorCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    2 x IFCCOVERING | object type "Plafond composé:Faux-Plafond Placostyl CF1h00" | CEILING | names: "Plafond composé:Faux-Plafond Placostyl CF1h00:5417407", "Plafond composé:Faux-Plafond Placostyl CF1h00:5417799" | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    34 x IFCCOLUMN | object type "Poteau RO (EN 10219-2):RO168.3x3" | names: "Poteau RO (EN 10219-2):RO168.3x3:5419546", "Poteau RO (EN 10219-2):RO168.3x3:5419561", "Poteau RO (EN 10219-2):RO168.3x3:5420455" (+31 more) | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn, Autre, Contraintes, Cotes
    3 x IFCBEAM | object type "Poutre - Lamellé-collé - Pin du sud:140 x 250" | names: "Poutre - Lamellé-collé - Pin du sud:140 x 250:5420760", "Poutre - Lamellé-collé - Pin du sud:140 x 250:5420778", "Poutre - Lamellé-collé - Pin du sud:140 x 250:5420808" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam, Autre, Contraintes, Cotes
    15 x IFCBEAM | object type "Poutre - Lamellé-collé - Pin du sud:76X140" | names: "Poutre - Lamellé-collé - Pin du sud:76X140:5421038", "Poutre - Lamellé-collé - Pin du sud:76X140:5421556", "Poutre - Lamellé-collé - Pin du sud:76X140:5421569" (+12 more) | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam, Autre, Contraintes, Cotes
    2 x IFCSLAB | object type "Sol:Finition béton peinture lessivable" | FLOOR | names: "Sol:Finition béton peinture lessivable:5430479", "Sol:Finition béton peinture lessivable:5432074" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Autre, Contraintes, Cotes
    4 x IFCBUILDINGELEMENTPROXY | object type "RPC Arbuste:Chitalpa Touffe 150" | names: "RPC Arbuste:Chitalpa Touffe 150:5445119", "RPC Arbuste:Chitalpa Touffe 150:5445154", "RPC Arbuste:Chitalpa Touffe 150:5445162" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Phase de construction, Données d'identification
    1 x IFCBUILDINGELEMENTPROXY | object type "RPC Arbre - Feuilles caduques:Arbre 1" | names: "RPC Arbre - Feuilles caduques:Arbre 1:5445857" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Phase de construction
    2 x IFCBUILDINGELEMENTPROXY | object type "RPC Arbre - Feuilles caduques:Mûrier 2" | names: "RPC Arbre - Feuilles caduques:Mûrier 2:5446103", "RPC Arbre - Feuilles caduques:Mûrier 2:5446113" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Données d'identification, Phase de construction
IFCBUILDINGSTOREY "Faux plafond" | long name "Faux plafond" | object type "Niveau:Ligne du Niveau" | elevation 154.1052
  contains 8 elements
    2 x IFCCOVERING | object type "Plafond composé:Faux-Plafond Placostyl CF1/2h00" | CEILING | names: "Plafond composé:Faux-Plafond Placostyl CF1/2h00:5095676", "Plafond composé:Faux-Plafond Placostyl CF1/2h00:5095700" | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    4 x IFCWALLSTANDARDCASE | object type "Mur de base:Bard bois vertical + MOB + contre cloison BA18" | names: "Mur de base:Bard bois vertical + MOB + contre cloison BA18:5131862", "Mur de base:Bard bois vertical + MOB + contre cloison BA18:5375789", "Mur de base:Bard bois vertical + MOB + contre cloison BA18:5376179" (+1 more) | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
    2 x IFCROOF | object type "Toit de base:tuile terre cuite" | names: "Toit de base:tuile terre cuite:5264992", "Toit de base:tuile terre cuite:5266239" | parts: 3 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon, Autre, Construction, Contraintes, Cotes
IFCBUILDINGSTOREY "N 01" | long name "N 01" | object type "Niveau:Ligne du Niveau" | elevation 154.66
  contains 2 elements
    1 x IFCWALLSTANDARDCASE | object type "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18" | names: "Mur de base:Bardage bois horizontal+ isolant+ MOB + contre cloison BA18:5177501" | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
    1 x IFCWALL | object type "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18" | names: "Mur de base:Enduit+ isolant +MOB + Contre cloison BA18:5177694" | property sets: Autre, Contraintes, Cotes, Données d'identification, Phase de construction, Structure
IFCBUILDINGSTOREY "Acrotère" | long name "Acrotère" | object type "Niveau:Ligne du Niveau" | elevation 155.3552
IFCBUILDINGSTOREY "Niveau acrotère garde corps" | long name "Niveau acrotère garde corps" | object type "Niveau:Ligne du Niveau" | elevation 156.1552
  contains 1 element
    1 x IFCROOF | object type "Toit de base:tuile terre cuite" | names: "Toit de base:tuile terre cuite:5100639" | parts: 4 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon, Autre, Construction, Contraintes, Cotes
IFCSPACE "-1/295" | long name "Rechauffage Dressage" | INTERNAL
  contains 2 elements
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5302119" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5371804" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
IFCSPACE "-1/289" | long name "Salle d'Activite Dortoir 2" | INTERNAL
  contains 26 elements
    1 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5360604" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
    25 x IFCFURNISHINGELEMENT | object type "Lit double - 02:Lit enfant 120x60" | names: "Lit double - 02:Lit enfant 120x60:5415628", "Lit double - 02:Lit enfant 120x60:5415629", "Lit double - 02:Lit enfant 120x60:5415747" (+22 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/288" | long name "Salle d'Activité Dortoir 1" | INTERNAL
  contains 24 elements
    2 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5360605", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5361429" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
    22 x IFCFURNISHINGELEMENT | object type "Lit double - 02:Lit enfant 120x60" | names: "Lit double - 02:Lit enfant 120x60:5415340", "Lit double - 02:Lit enfant 120x60:5415553", "Lit double - 02:Lit enfant 120x60:5415561" (+19 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/287" | long name "CHANGE" | INTERNAL
IFCSPACE "-1/285" | long name "Accès self" | INTERNAL
  contains 3 elements
    3 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5371013", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5371021", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5436479" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/283" | long name "Preparation" | INTERNAL
  contains 1 element
    1 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372781" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/281" | long name "Salle d'Activité 11" | INTERNAL
  contains 3 elements
    3 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5356566", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5356567", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5356569" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/280" | long name "Salle d'activité 10" | INTERNAL
  contains 4 elements
    4 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5356576", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5356577", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5356578" (+1 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
IFCSPACE "-1/279" | long name "Salle d'activité RAM" | INTERNAL
IFCSPACE "-1/276" | long name "Salle de Pause" | INTERNAL
  contains 2 elements
    2 x IFCFURNISHINGELEMENT | object type "Casier:Sloped Roof Cabinet 1861x300x400" | names: "Casier:Sloped Roof Cabinet 1861x300x400:5333039", "Casier:Sloped Roof Cabinet 1861x300x400:5333047" | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Construction, Contraintes, Cotes
IFCSPACE "-1/270" | long name "CTA RAM ACCUEIL" | INTERNAL
  contains 1 element
    1 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5360586" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
IFCSPACE "-1/268" | long name "Sanitaires Personnel" | INTERNAL
  contains 4 elements
    1 x IFCBUILDINGELEMENTPROXY | object type "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC" | names: "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5348913" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5348914" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5348915" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5348917" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
IFCSPACE "-1/267" | long name "Vestiaires F" | INTERNAL
IFCSPACE "-1/266" | long name "Salle de Pause" | INTERNAL
IFCSPACE "-1/264" | long name "Circulation Self et Dépose Plateau" | INTERNAL
  contains 3 elements
    3 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5370999", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5371033", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372791" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/263" | long name "Salle de Restauration 3 -6/12 ans self Service" | INTERNAL
  contains 64 elements
    7 x IFCFURNISHINGELEMENT | object type "Table de cuisine:80 x 150 x 75 cm" | names: "Table de cuisine:80 x 150 x 75 cm:5177091", "Table de cuisine:80 x 150 x 75 cm:5177099", "Table de cuisine:80 x 150 x 75 cm:5177113" (+4 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
    14 x IFCFURNISHINGELEMENT | object type "Chaise bois - 01:Chaise bois - rouge" | names: "Chaise bois - 01:Chaise bois - rouge:5177092", "Chaise bois - 01:Chaise bois - rouge:5177095", "Chaise bois - 01:Chaise bois - rouge:5177100" (+11 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    20 x IFCFURNISHINGELEMENT | object type "Chaise bois - 01:Chaise bois - vert" | names: "Chaise bois - 01:Chaise bois - vert:5177093", "Chaise bois - 01:Chaise bois - vert:5177096", "Chaise bois - 01:Chaise bois - vert:5177101" (+17 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    20 x IFCFURNISHINGELEMENT | object type "Chaise bois - 01:Chaise bois - jaune" | names: "Chaise bois - 01:Chaise bois - jaune:5177094", "Chaise bois - 01:Chaise bois - jaune:5177097", "Chaise bois - 01:Chaise bois - jaune:5177102" (+17 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    3 x IFCFURNISHINGELEMENT | object type "Table de cuisine:80 x 100 x 75 cm 2" | names: "Table de cuisine:80 x 100 x 75 cm 2:5177107", "Table de cuisine:80 x 100 x 75 cm 2:5177129", "Table de cuisine:80 x 100 x 75 cm 2:5177150" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/258" | long name "Local Poubelles" | INTERNAL
  contains 1 element
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5177246" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
IFCSPACE "-1/257" | long name "Plonge/ Stockage" | INTERNAL
  contains 2 elements
    2 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372634", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372771" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/255" | long name "Salle de restauration 4 - 6/12 ans self service" | INTERNAL
  contains 56 elements
    8 x IFCFURNISHINGELEMENT | object type "Table de cuisine:80 x 150 x 75 cm" | names: "Table de cuisine:80 x 150 x 75 cm:5177168", "Table de cuisine:80 x 150 x 75 cm:5177176", "Table de cuisine:80 x 150 x 75 cm:5177185" (+5 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
    16 x IFCFURNISHINGELEMENT | object type "Chaise bois - 01:Chaise bois - rouge" | names: "Chaise bois - 01:Chaise bois - rouge:5177169", "Chaise bois - 01:Chaise bois - rouge:5177172", "Chaise bois - 01:Chaise bois - rouge:5177177" (+13 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    16 x IFCFURNISHINGELEMENT | object type "Chaise bois - 01:Chaise bois - vert" | names: "Chaise bois - 01:Chaise bois - vert:5177170", "Chaise bois - 01:Chaise bois - vert:5177173", "Chaise bois - 01:Chaise bois - vert:5177178" (+13 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    16 x IFCFURNISHINGELEMENT | object type "Chaise bois - 01:Chaise bois - jaune" | names: "Chaise bois - 01:Chaise bois - jaune:5177171", "Chaise bois - 01:Chaise bois - jaune:5177174", "Chaise bois - 01:Chaise bois - jaune:5177179" (+13 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
IFCSPACE "-1/251" | long name "Local entretien" | INTERNAL
IFCSPACE "-1/247" | long name "Sanitaires G." | INTERNAL
  contains 16 elements
    4 x IFCBUILDINGELEMENTPROXY | object type "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC" | names: "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5333687", "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5333690", "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5333693" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    4 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5333688", "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5333691", "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5333694" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    4 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5333689", "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5333692", "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5333695" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    2 x IFCFLOWTERMINAL | object type "Urinoir:Urinoir" | names: "Urinoir:Urinoir:5334670", "Urinoir:Urinoir:5334822" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    2 x IFCFLOWTERMINAL | object type "Lavabo mural - 09:1000mm x 462mm" | names: "Lavabo mural - 09:1000mm x 462mm:5337955", "Lavabo mural - 09:1000mm x 462mm:5337989" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
IFCSPACE "-1/243" | long name "Salle Activité 9" | INTERNAL
IFCSPACE "-1/241" | long name "Circulation 6/12" | INTERNAL
  contains 11 elements
    7 x IFCFURNISHINGELEMENT | object type "Etagère:Rack cartable" | names: "Etagère:Rack cartable:5316460", "Etagère:Rack cartable:5316984", "Etagère:Rack cartable:5316998" (+4 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
    4 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358158", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358159", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358160" (+1 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/237" | long name "Salle Activité 7" | INTERNAL | description "Espace 6/12 ans"
IFCSPACE "-1/236" | long name "Local Poubelle" | INTERNAL
IFCSPACE "-1/232" | long name "Salle Activité 12" | INTERNAL
IFCSPACE "-1/230" | long name "Circulation 3/6" | INTERNAL
  contains 15 elements
    7 x IFCFURNISHINGELEMENT | object type "Etagère:Rack cartable" | names: "Etagère:Rack cartable:5317020", "Etagère:Rack cartable:5317034", "Etagère:Rack cartable:5317046" (+4 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
    8 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359366", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359367", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359368" (+5 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/229" | long name "Salle Activité 2" | INTERNAL
IFCSPACE "-1/228" | long name "Salle Activité 4" | INTERNAL
IFCSPACE "-1/227" | long name "Salle Activité 3" | INTERNAL
  contains 4 elements
    4 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359356", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359357", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359358" (+1 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/220" | long name "Salle Activité13" | INTERNAL
  contains 2 elements
    2 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358103", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5358104" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/215" | long name "Salle Activité 6" | INTERNAL
  contains 4 elements
    4 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359361", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359362", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359363" (+1 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/214" | long name "Salle Activité 5" | INTERNAL
IFCSPACE "-1/210" | long name "Sanitaires 2" | INTERNAL
  contains 16 elements
    9 x IFCBUILDINGELEMENTPROXY | object type "WC enfant:Default" | names: "WC enfant:Default:5342065", "WC enfant:Default:5342176", "WC enfant:Default:5342184" (+6 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
    3 x IFCFLOWTERMINAL | object type "Lavabo mural - 09:1000mm x 462mm" | names: "Lavabo mural - 09:1000mm x 462mm:5343045", "Lavabo mural - 09:1000mm x 462mm:5343082", "Lavabo mural - 09:1000mm x 462mm:5343123" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    4 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5360602", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5360603", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5361137" (+1 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/204" | long name "Sanitaires" | INTERNAL
IFCSPACE "-1/198" | long name "Salle Activité 1" | INTERNAL | description "Espace 3/6 ans"
IFCSPACE "-1/197" | long name "San. mixte 3/6 ans" | INTERNAL | description "Salle de restauration"
  contains 1 element
    1 x IFCBUILDINGELEMENTPROXY | object type "WC enfant:Default" | names: "WC enfant:Default:5436150" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
IFCSPACE "-1/168" | long name "Sanitaires G." | INTERNAL | description "Salle de restauration"
  contains 3 elements
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5434040" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5434041" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5434145" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
IFCSPACE "-1/151" | long name "Sanitaires F." | INTERNAL | description "Salle de restauration"
  contains 2 elements
    2 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372446", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372576" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/150" | long name "Sanitaires F." | INTERNAL | description "Espace 6/12 ans"
  contains 21 elements
    5 x IFCBUILDINGELEMENTPROXY | object type "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC" | names: "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5333544", "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5333637", "PB WC sur pied:E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC:5333647" (+2 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    5 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5333545", "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5333638", "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5333648" (+2 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    5 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5333546", "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5333639", "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5333649" (+2 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    2 x IFCFLOWTERMINAL | object type "Lavabo mural - 09:1000mm x 462mm" | names: "Lavabo mural - 09:1000mm x 462mm:5338117", "Lavabo mural - 09:1000mm x 462mm:5338118" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    4 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5347776", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5347777", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5347778" (+1 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction, Données d'identification
IFCSPACE "-1/135" | long name "Stock froid/sec" | INTERNAL | description "Cuisines"
  contains 4 elements
    1 x IFCBUILDINGELEMENTPROXY | object type "Congélateur - Vertical:1000mm x 1000mm" | names: "Congélateur - Vertical:1000mm x 1000mm:5176940" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    2 x IFCBUILDINGELEMENTPROXY | object type "Réfrigérateur double porte:double porte 1500 x 1000" | names: "Réfrigérateur double porte:double porte 1500 x 1000:5176941", "Réfrigérateur double porte:double porte 1500 x 1000:5176942" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Electricité - Charges
    1 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5371928" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
IFCSPACE "-1/130" | long name "Vestiaires H" | INTERNAL | description "Locaux personnel"
  contains 1 element
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5352047" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
IFCSPACE "-1/121" | long name "Sas d'Accueil" | INTERNAL | description "Salle de restauration"
  contains 1 element
    1 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5370658" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
IFCSPACE "-1/120" | long name "Sas thermique" | INTERNAL | description "Circulations"
  contains 4 elements
    4 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5370952", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372209", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5372386" (+1 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/119" | long name "Salle de restauration 1 & 2 - 3/6 ans service à table" | INTERNAL | description "Salle de restauration"
  contains 126 elements
    36 x IFCFURNISHINGELEMENT | object type "Chaise enfant 3-6:Chaise enfant jaune" | names: "Chaise enfant 3-6:Chaise enfant jaune:5176947", "Chaise enfant 3-6:Chaise enfant jaune:5176951", "Chaise enfant 3-6:Chaise enfant jaune:5176955" (+33 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    36 x IFCFURNISHINGELEMENT | object type "Chaise enfant 3-6:Chaise enfant bleu" | names: "Chaise enfant 3-6:Chaise enfant bleu:5176948", "Chaise enfant 3-6:Chaise enfant bleu:5176952", "Chaise enfant 3-6:Chaise enfant bleu:5176956" (+33 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    36 x IFCFURNISHINGELEMENT | object type "Chaise enfant 3-6:Chaise enfant vert" | names: "Chaise enfant 3-6:Chaise enfant vert:5176949", "Chaise enfant 3-6:Chaise enfant vert:5176950", "Chaise enfant 3-6:Chaise enfant vert:5176957" (+33 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    18 x IFCFURNISHINGELEMENT | object type "Table ronde enfants:Diamètre de 1100 mm" | names: "Table ronde enfants:Diamètre de 1100 mm:5176953", "Table ronde enfants:Diamètre de 1100 mm:5176961", "Table ronde enfants:Diamètre de 1100 mm:5176969" (+15 more) | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/111" | long name "Sanitaires 1" | INTERNAL | description "Espace 3/6 ans"
  contains 16 elements
    10 x IFCBUILDINGELEMENTPROXY | object type "WC enfant:Default" | names: "WC enfant:Default:5343217", "WC enfant:Default:5343218", "WC enfant:Default:5343219" (+7 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Phase de construction
    3 x IFCFLOWTERMINAL | object type "Lavabo mural - 09:1000mm x 462mm" | names: "Lavabo mural - 09:1000mm x 462mm:5343465", "Lavabo mural - 09:1000mm x 462mm:5343495", "Lavabo mural - 09:1000mm x 462mm:5343547" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    3 x IFCFURNISHINGELEMENT | object type "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default" | names: "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359342", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359343", "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000:Default:5359345" | property sets: Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification, Phase de construction
IFCSPACE "-1/95" | long name "Lingerie" | INTERNAL | description "Locaux entretien"
IFCSPACE "-1/86" | long name "Bureau Inscription" | INTERNAL | description "Administration personnel"
IFCSPACE "-1/70" | long name "Salles Activité 8" | INTERNAL | description "Espace 6/12 ans"
IFCSPACE "-1/62" | long name "Sanitaires H." | INTERNAL | description "Salle polyvalente"
  contains 3 elements
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5338387" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5338388" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5340473" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
IFCSPACE "-1/61" | long name "Sanitaires F" | INTERNAL | description "Salle polyvalente"
  contains 2 elements
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5338267" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5338268" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
IFCSPACE "-1/59" | long name "Sanitaires Personnel H." | INTERNAL | description "Administration personnel"
  contains 3 elements
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5340602" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5347864" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5347865" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
IFCSPACE "-1/58" | long name "Sanitaires Personnel F." | INTERNAL | description "Administration personnel"
  contains 3 elements
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5340559" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" | names: "POR_Multisuite_P5045_BIM_FR:P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC:5347861" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
    1 x IFCBUILDINGELEMENTPROXY | object type "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC" | names: "POR_Ulysse_E9034_BIM_FR:E903401 - ULYSSE RES,DC AL LAT BLANC:5347862" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes
IFCSPACE "-1/51" | long name "Bureau Directeur" | INTERNAL | description "Administration personnel"
IFCSPACE "-1/50" | long name "Infirmerie" | INTERNAL | description "Administration personnel"
IFCSPACE "-1/48" | long name "Casiers Personnel" | INTERNAL | description "Administration personnel"
  contains 18 elements
    18 x IFCFURNISHINGELEMENT | object type "Casier:Sloped Roof Cabinet 1861x300x400" | names: "Casier:Sloped Roof Cabinet 1861x300x400:5332776", "Casier:Sloped Roof Cabinet 1861x300x400:5332935", "Casier:Sloped Roof Cabinet 1861x300x400:5332943" (+15 more) | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Construction, Contraintes, Cotes
IFCSPACE "-1/47" | long name "Bureau des Animateurs" | INTERNAL | description "Administration personnel"
IFCSPACE "-1/46" | long name "Local Vidoir" | INTERNAL | description "Locaux entretien"
IFCSPACE "-1/45" | long name "Vestiaire Entretien" | INTERNAL | description "Locaux entretien"
  contains 1 element
    1 x IFCFLOWTERMINAL | object type "Lavabo sur console métallique:Lave main cuisine" | names: "Lavabo sur console métallique:Lave main cuisine:5340512" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Autre, Contraintes, Cotes, Données d'identification

Property sets
  Données d'identification | properties | on 252 objects (129 IFCWALLSTANDARDCASE, 79 IFCFURNISHINGELEMENT, 12 IFCBUILDINGELEMENTPROXY, 8 IFCMEMBER)
    Variantes = "Modèle de base" (IFCTEXT)
  Données d'identification | properties | on 57 objects (57 IFCFURNISHINGELEMENT)
    Nom de l'assemblage = "table 6" (IFCTEXT)
  Données d'identification | properties | on 48 objects (48 IFCFURNISHINGELEMENT)
    Nom de l'assemblage = "table 6" (IFCTEXT)
    Variantes = "Modèle de base" (IFCTEXT)
  Données d'identification | properties | on 40 objects (40 IFCFURNISHINGELEMENT)
    Nom de l'assemblage = "Mobilier 005" (IFCTEXT)
  Données d'identification | properties | on 34 objects (22 IFCCOLUMN, 12 IFCBEAM)
    Commentaires = "" (IFCTEXT)
  Données d'identification | properties | on 32 objects (32 IFCFURNISHINGELEMENT)
    Nom de l'assemblage = "table enfant ronde 6" (IFCTEXT)
    Variantes = "Modèle de base" (IFCTEXT)
  Données d'identification | properties | on 31 objects (31 IFCFURNISHINGELEMENT)
    Nom de l'assemblage = "table enfant ronde 6" (IFCTEXT)
  Données d'identification | properties | on 26 objects (16 IFCCOLUMN, 10 IFCBEAM)
    Commentaires = "" (IFCTEXT)
    Variantes = "Modèle de base" (IFCTEXT)
  Données d'identification: 387 more contents on 520 objects not shown
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Reference = "Surface local ext 1 4" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    CeilingCovering = "CF 1/2h +Ecophon Hygiène" (IFCLABEL)
    FloorCovering = "Sol souple PVC" (IFCLABEL)
    Reference = "Vestiaire Entretien -1/45" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    CeilingCovering = "CF 1/2h + Ecophon" (IFCLABEL)
    FloorCovering = "Linoleum Hyacinth" (IFCLABEL)
    Reference = "Local Vidoir -1/46" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    CeilingCovering = "CF 1/2h + Ecophon" (IFCLABEL)
    FloorCovering = "Linoleum Hyacinth" (IFCLABEL)
    Reference = "Bureau des Animateurs -1/47" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    CeilingCovering = "CF 1/2h + Ecophon" (IFCLABEL)
    FloorCovering = "Linoleum Hyacinth" (IFCLABEL)
    Reference = "Casiers Personnel -1/48" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    CeilingCovering = "CF 1/2h + Organic35" (IFCLABEL)
    FloorCovering = "Linoleum Hyacinth" (IFCLABEL)
    Reference = "Accueil Commun -1/49" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    CeilingCovering = "CF 1/2h + Ecophon" (IFCLABEL)
    FloorCovering = "Linoleum Hyacinth" (IFCLABEL)
    Reference = "Infirmerie -1/50" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    CeilingCovering = "CF 1/2h + Ecophon" (IFCLABEL)
    FloorCovering = "Linoleum Hyacinth" (IFCLABEL)
    Reference = "Bureau Directeur -1/51" (IFCIDENTIFIER)
  Pset_SpaceCommon: 95 more contents on 95 objects not shown
  Analyse d'énergie | properties | on 91 objects (91 IFCSPACE)
    Charge d'éclairage basse sur = "Par type d'espace" (IFCIDENTIFIER)
    Charge d'éclairage réelle par surface = 0. (IFCREAL)
    Charge d'éclairage spécifiée = 0. (IFCPOWERMEASURE) [WATT]
    Charge d'éclairage spécifiée par surface = 15.0694745833936 (IFCREAL)
    Charge de puissance basse sur = "Par type d'espace" (IFCIDENTIFIER)
    Charge de puissance réelle = 0. (IFCPOWERMEASURE) [WATT]
    Charge de puissance réelle par surface = 0. (IFCREAL)
    Charge de puissance spécifiée = 0. (IFCPOWERMEASURE) [WATT]
    Charge de puissance spécifiée par surface = 18.2986477084065 (IFCREAL)
    Charge réelle d'éclairage = 0. (IFCPOWERMEASURE) [WATT]
    Contribution à l'éclairage du plénum = 0.2 (IFCREAL)
    Gain de chaleur latente par personne = 1498.43060390495 (IFCREAL)
    Gain de chaleur perceptible par personne = 867.512454892338 (IFCREAL)
    Gain de chaleur total par personne = 2365.94305879729 (IFCREAL)
    Nombre de personnes = 0. (IFCREAL)
    Surface par personne = 10. (IFCAREAMEASURE) [SQUARE_METRE]
    Unités de charge d'éclairage = "Densité de puissance" (IFCIDENTIFIER)
    Unités de charge de puissance = "Densité de puissance" (IFCIDENTIFIER)
    Valeurs de charge de chauffage = "Par type d'espace" (IFCIDENTIFIER)
  Autre | properties | on 110 objects (106 IFCWALLSTANDARDCASE, 4 IFCWALL)
    Catégorie = "Murs" (IFCLABEL)
    Famille = "Mur de base: 84/48 BA18 isol 45" (IFCLABEL)
    Famille et type = "Mur de base: 84/48 BA18 isol 45" (IFCLABEL)
    ID du type = "Mur de base: 84/48 BA18 isol 45" (IFCLABEL)
    Type = "Mur de base: 84/48 BA18 isol 45" (IFCLABEL)
  Autre | properties | on 83 objects (83 IFCFURNISHINGELEMENT)
    BOS_TR_IDENTITY_dx = 0. (IFCREAL)
    BOS_TR_IDENTITY_dy = 0. (IFCREAL)
    BOS_TR_IDENTITY_dz = 0. (IFCREAL)
    BOS_TR_IDENTITY_rx = 0. (IFCREAL)
    BOS_TR_IDENTITY_ry = 0. (IFCREAL)
    BOS_TR_IDENTITY_rz = 0. (IFCREAL)
    BOS_TR_IDENTITY_sx = 1. (IFCREAL)
    BOS_TR_IDENTITY_sy = 1. (IFCREAL)
    BOS_TR_IDENTITY_sz = 1. (IFCREAL)
    Catégorie = "Mobilier" (IFCLABEL)
    Famille = "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000: Default" (IFCLABEL)
    Famille et type = "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000: Default" (IFCLABEL)
    ID du type = "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000: Default" (IFCLABEL)
    Type = "Furniture_Shelving-Storage_Dalform_Hook-Strip-1000: Default" (IFCLABEL)
  Autre | properties | on 59 objects (59 IFCSPACE)
    Catégorie = "Pièces" (IFCLABEL)
    ID de phase = "Nouvelle construction" (IFCLABEL)
  Autre | properties | on 47 objects (47 IFCFURNISHINGELEMENT)
    Catégorie = "Mobilier" (IFCLABEL)
    Famille = "Lit double - 02: Lit enfant 120x60" (IFCLABEL)
    Famille et type = "Lit double - 02: Lit enfant 120x60" (IFCLABEL)
    ID du type = "Lit double - 02: Lit enfant 120x60" (IFCLABEL)
    Type = "Lit double - 02: Lit enfant 120x60" (IFCLABEL)
  Autre | properties | on 38 objects (38 IFCWALLSTANDARDCASE)
    Catégorie = "Murs" (IFCLABEL)
    Famille = "Mur de base: Refend MOB 16 cm+ contre cloison BA18" (IFCLABEL)
    Famille et type = "Mur de base: Refend MOB 16 cm+ contre cloison BA18" (IFCLABEL)
    ID du type = "Mur de base: Refend MOB 16 cm+ contre cloison BA18" (IFCLABEL)
    Type = "Mur de base: Refend MOB 16 cm+ contre cloison BA18" (IFCLABEL)
  Autre | properties | on 36 objects (36 IFCFURNISHINGELEMENT)
    Catégorie = "Mobilier" (IFCLABEL)
    Famille = "Chaise enfant 3-6: Chaise enfant jaune" (IFCLABEL)
    Famille et type = "Chaise enfant 3-6: Chaise enfant jaune" (IFCLABEL)
    ID du type = "Chaise enfant 3-6: Chaise enfant jaune" (IFCLABEL)
    Type = "Chaise enfant 3-6: Chaise enfant jaune" (IFCLABEL)
  Autre | properties | on 36 objects (36 IFCFURNISHINGELEMENT)
    Catégorie = "Mobilier" (IFCLABEL)
    Famille = "Chaise enfant 3-6: Chaise enfant bleu" (IFCLABEL)
    Famille et type = "Chaise enfant 3-6: Chaise enfant bleu" (IFCLABEL)
    ID du type = "Chaise enfant 3-6: Chaise enfant bleu" (IFCLABEL)
    Type = "Chaise enfant 3-6: Chaise enfant bleu" (IFCLABEL)
  Autre | properties | on 36 objects (36 IFCFURNISHINGELEMENT)
    Catégorie = "Mobilier" (IFCLABEL)
    Famille = "Chaise enfant 3-6: Chaise enfant vert" (IFCLABEL)
    Famille et type = "Chaise enfant 3-6: Chaise enfant vert" (IFCLABEL)
    ID du type = "Chaise enfant 3-6: Chaise enfant vert" (IFCLABEL)
    Type = "Chaise enfant 3-6: Chaise enfant vert" (IFCLABEL)
  Autre: 143 more contents on 847 objects not shown
  Contraintes | properties | on 291 objects (251 IFCFURNISHINGELEMENT, 29 IFCBUILDINGELEMENTPROXY, 11 IFCFLOWTERMINAL)
    Décalage = 0. (IFCLENGTHMEASURE) [METRE]
    Hôte = "Niveau : N 00" (IFCTEXT)
    Niveau = "Niveau: N 00" (IFCLABEL)
    Se déplace avec les éléments voisins = FALSE (IFCBOOLEAN)
  Contraintes | properties | on 141 objects (116 IFCDOOR, 25 IFCOPENINGELEMENT)
    Hauteur de l'appui = 0. (IFCLENGTHMEASURE) [METRE]
    Niveau = "Niveau: N 00" (IFCLABEL)
  Contraintes | properties | on 80 objects (78 IFCFURNISHINGELEMENT, 2 IFCBUILDINGELEMENTPROXY)
    Hôte = "Niveau : N 00" (IFCTEXT)
    Niveau = "Niveau: N 00" (IFCLABEL)
    Se déplace avec les éléments voisins = FALSE (IFCBOOLEAN)
  Contraintes | properties | on 43 objects (42 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Contrainte inférieure = "Niveau: N 00" (IFCLABEL)
    Décalage inférieur = 0. (IFCLENGTHMEASURE) [METRE]
    Décalage supérieur = 0. (IFCLENGTHMEASURE) [METRE]
    Extension inférieure = 0. (IFCLENGTHMEASURE) [METRE]
    Extension supérieure = 0. (IFCLENGTHMEASURE) [METRE]
    Hauteur non contrainte = 2.8 (IFCLENGTHMEASURE) [METRE]
    Ligne de justification = "Axe du mur" (IFCIDENTIFIER)
    Limite de pièce = TRUE (IFCBOOLEAN)
    Lié au volume = FALSE (IFCBOOLEAN)
    Partie inférieure attachée = FALSE (IFCBOOLEAN)
    Partie supérieure attachée = FALSE (IFCBOOLEAN)
  Contraintes | properties | on 39 objects (39 IFCFURNISHINGELEMENT)
    Décalage = 0.8 (IFCLENGTHMEASURE) [METRE]
    Hôte = "Niveau : N 00" (IFCTEXT)
    Niveau = "Niveau: N 00" (IFCLABEL)
    Se déplace avec les éléments voisins = FALSE (IFCBOOLEAN)
  Contraintes | properties | on 36 objects (36 IFCSPACE)
    Décalage inférieur = 0. (IFCLENGTHMEASURE) [METRE]
    Décalage limite = 2.4384 (IFCLENGTHMEASURE) [METRE]
    Limite supérieure = "Niveau: N 00" (IFCLABEL)
    Niveau = "Niveau: N 00" (IFCLABEL)
  Contraintes | properties | on 35 objects (35 IFCWINDOW)
    Hauteur de l'appui = 0.4 (IFCLENGTHMEASURE) [METRE]
    Niveau = "Niveau: N 00" (IFCLABEL)
  Contraintes | properties | on 34 objects (34 IFCSPACE)
    Décalage inférieur = 0. (IFCLENGTHMEASURE) [METRE]
    Décalage limite = 2.4384 (IFCLENGTHMEASURE) [METRE]
    Limite supérieure = "Niveau: N 00" (IFCLABEL)
    Niveau = "N 00" (IFCTEXT)
  Contraintes: 132 more contents on 554 objects not shown
  Cotes | properties | on 108 objects (108 IFCFURNISHINGELEMENT)
    Surface = 0.315900174966141 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00373810312885813 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 102 objects (102 IFCFURNISHINGELEMENT)
    Surface = 0.477515862536313 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00614739079067027 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 83 objects (83 IFCFURNISHINGELEMENT)
    Surface = 0.442573878048333 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0179163034716757 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 47 objects (47 IFCFURNISHINGELEMENT)
    Surface = 2.40407714600106 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.303714711653585 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 31 objects (31 IFCWINDOW)
    Surface = 5.23275 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.107325000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 24 objects (18 IFCDOOR, 6 IFCOPENINGELEMENT)
    Surface = 2.76925000000512 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0958830000001831 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 24 objects (22 IFCDOOR, 2 IFCOPENINGELEMENT)
    Surface = 2.74999999999991 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0395874999999998 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 22 objects (22 IFCFURNISHINGELEMENT)
    Base Height = 0.2 (IFCLENGTHMEASURE) [METRE]
    Surface = 26.7578175298586 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.35887032334379 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes: 530 more contents on 792 objects not shown
  Phase de construction | properties | on 1174 objects (413 IFCFURNISHINGELEMENT, 267 IFCWALLSTANDARDCASE, 121 IFCDOOR, 77 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Phase de construction | properties | on 91 objects (91 IFCSPACE)
    Phase = "Nouvelle construction" (IFCLABEL)
  Structure | properties | on 277 objects (267 IFCWALLSTANDARDCASE, 8 IFCWALL, 2 IFCCURTAINWALL)
    Activer le modèle analytique = FALSE (IFCBOOLEAN)
    Structure = FALSE (IFCBOOLEAN)
    Utilisation structurelle = "Non porteur" (IFCIDENTIFIER)
  Structure | properties | on 42 objects (42 IFCCOLUMN)
    Activer le modèle analytique = TRUE (IFCBOOLEAN)
  Structure | properties | on 16 objects (16 IFCSLAB)
    Activer le modèle analytique = FALSE (IFCBOOLEAN)
    Structure = FALSE (IFCBOOLEAN)
  Structure | properties | on 2 objects (2 IFCSTAIR)
    Enrobage d'armature = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
  Structure | properties | on 1 object (1 IFCBEAM)
    Activer le modèle analytique = TRUE (IFCBOOLEAN)
    Enrobage d'armature - Autres faces = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face inférieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face supérieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Longueur de coupe = 3.6934 (IFCLENGTHMEASURE) [METRE]
    Utilisation structurelle = "Autre" (IFCIDENTIFIER)
  Structure | properties | on 1 object (1 IFCBEAM)
    Activer le modèle analytique = TRUE (IFCBOOLEAN)
    Enrobage d'armature - Autres faces = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face inférieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face supérieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Longueur de coupe = 7.9144759721016 (IFCLENGTHMEASURE) [METRE]
    Utilisation structurelle = "Autre" (IFCIDENTIFIER)
  Structure | properties | on 1 object (1 IFCBEAM)
    Activer le modèle analytique = TRUE (IFCBOOLEAN)
    Enrobage d'armature - Autres faces = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face inférieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face supérieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Longueur de coupe = 3.5074 (IFCLENGTHMEASURE) [METRE]
    Utilisation structurelle = "Autre" (IFCIDENTIFIER)
  Structure | properties | on 1 object (1 IFCBEAM)
    Activer le modèle analytique = TRUE (IFCBOOLEAN)
    Enrobage d'armature - Autres faces = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face inférieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Enrobage d'armature - Face supérieure = "Paramètres de l'enrobage d'armature: Enrobage d'armature 1" (IFCLABEL)
    Longueur de coupe = 6.67320563487337 (IFCLENGTHMEASURE) [METRE]
    Utilisation structurelle = "Autre" (IFCIDENTIFIER)
  Structure: 18 more contents on 18 objects not shown
  Pset_QuantityTakeOff | properties | on 124 objects (106 IFCWALLSTANDARDCASE, 14 IFCOPENINGELEMENT, 4 IFCWALL)
    Reference = "84/48 BA18 isol 45" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 103 objects (83 IFCFURNISHINGELEMENT, 20 IFCBUILDINGELEMENTPROXY)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 53 objects (38 IFCWALLSTANDARDCASE, 15 IFCOPENINGELEMENT)
    Reference = "Refend MOB 16 cm+ contre cloison BA18" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 47 objects (47 IFCFURNISHINGELEMENT)
    Reference = "Lit enfant 120x60" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 36 objects (36 IFCFURNISHINGELEMENT)
    Reference = "Chaise enfant jaune" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 36 objects (36 IFCFURNISHINGELEMENT)
    Reference = "Chaise enfant bleu" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 36 objects (36 IFCFURNISHINGELEMENT)
    Reference = "Chaise enfant vert" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 36 objects (36 IFCFURNISHINGELEMENT)
    Reference = "Chaise bois - vert" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 88 more contents on 722 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 110 objects (106 IFCWALLSTANDARDCASE, 4 IFCWALL)
    Description = "Type 98/48" (IFCTEXT)
    Reference = "84/48 BA18 isol 45" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 38 objects (38 IFCWALLSTANDARDCASE)
    Reference = "Refend MOB 16 cm+ contre cloison BA18" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 34 objects (34 IFCWALLSTANDARDCASE)
    Reference = "Séparation sanitaires 3/6" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 24 objects (21 IFCWALLSTANDARDCASE, 3 IFCWALL)
    Reference = "Enduit+ isolant +MOB + Contre cloison BA18" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    Reference = "Bard bois vertical + MOB + contre cloison BA18" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    Reference = "Cloison mobile à galandage" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    Reference = "Acrotère - enduit 2 + isolant 12 + MOB + enduit" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 10 objects (9 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Reference = "Bardage bois horizontal+ isolant+ MOB + contre cloison BA18" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 2 more contents on 11 objects not shown
  Pset_WallCommon | properties | on 110 objects (106 IFCWALLSTANDARDCASE, 4 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "84/48 BA18 isol 45" (IFCIDENTIFIER)
    ThermalTransmittance = 25. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 36 objects (36 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Refend MOB 16 cm+ contre cloison BA18" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 34 objects (34 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Séparation sanitaires 3/6" (IFCIDENTIFIER)
    ThermalTransmittance = 26.15 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 24 objects (21 IFCWALLSTANDARDCASE, 3 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Enduit+ isolant +MOB + Contre cloison BA18" (IFCIDENTIFIER)
    ThermalTransmittance = 36.1111111111111 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Bard bois vertical + MOB + contre cloison BA18" (IFCIDENTIFIER)
    ThermalTransmittance = 1.44017725258493 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Cloison mobile à galandage" (IFCIDENTIFIER)
    ThermalTransmittance = 25. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 11 objects (11 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Acrotère - enduit 2 + isolant 12 + MOB + enduit" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 10 objects (9 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Bardage bois horizontal+ isolant+ MOB + contre cloison BA18" (IFCIDENTIFIER)
    ThermalTransmittance = 4.44444444444444 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 5 more contents on 18 objects not shown
  Graphismes | properties | on 48 objects (39 IFCDOOR, 9 IFCOPENINGELEMENT)
    Angle d'ouverture 2D fixe = TRUE (IFCBOOLEAN)
    Angle d'ouverture 3D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Graphismes | properties | on 22 objects (21 IFCDOOR, 1 IFCOPENINGELEMENT)
    Angle d'ouverture (à droite) = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle d'ouverture (à gauche) = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle d'ouverture 2D fixe = TRUE (IFCBOOLEAN)
  Graphismes | properties | on 4 objects (2 IFCDOOR, 2 IFCOPENINGELEMENT)
    Angle d'ouverture 2D fixé = TRUE (IFCBOOLEAN)
    Angle d'ouverture = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle d'ouverture G = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Graphismes | properties | on 4 objects (4 IFCWINDOW)
    Encadrement intérieur = FALSE (IFCBOOLEAN)
  Graphismes | properties | on 3 objects (3 IFCWINDOW)
    A battant = TRUE (IFCBOOLEAN)
    A soufflet = TRUE (IFCBOOLEAN)
    Encadrement intérieur = FALSE (IFCBOOLEAN)
  Pset_OpeningElementCommon | properties | on 15 objects (15 IFCOPENINGELEMENT)
    Reference = "Refend MOB 16 cm+ contre cloison BA18" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 14 objects (14 IFCOPENINGELEMENT)
    Reference = "84/48 BA18 isol 45" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 6 objects (6 IFCOPENINGELEMENT)
    Reference = "Bard bois vertical + MOB + contre cloison BA18" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 3 objects (3 IFCOPENINGELEMENT)
    Reference = "Enduit+ isolant +MOB + Contre cloison BA18" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Reference = "Bardage bois horizontal+ isolant+ MOB + contre cloison BA18" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Reference = "Acrotère - enduit 2 + isolant 12 + MOB + enduit" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Séparation sanitaires 3/6" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 32 objects (32 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "92x204" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 22 objects (22 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "205x105" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 16 objects (16 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "183x204cm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 8 objects (8 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Placard coulissante - 3 panneaux 3m80" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "205x210" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "82x204" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 5 objects (5 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "143x229cm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Placard coulissante - 3 panneaux 4m" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon: 11 more contents on 20 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 220 objects (210 IFCFURNISHINGELEMENT, 10 IFCFLOWTERMINAL)
    Manufacturer (no value)
  Pset_ManufacturerTypeInformation | properties | on 45 objects (45 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "sav@idealstandard.com" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 22 objects (22 IFCFURNISHINGELEMENT)
    Manufacturer = "Sonneson Inredningar" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCSLAB)
    Manufacturer = "Tarkett" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    Manufacturer = "ALTO PRODUCTION" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Groupe SAFIR" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 15 objects (15 IFCSLAB)
    Reference = "tuile terre cuite" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "Enrobé végétaux a froid" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Dalle en béton 20 + iso 10" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Aire de jeux sol souple ext" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Finition béton peinture lessivable" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Description = "Le revêtement de sol sélectionné du type Linosom Silencio xf™2 (décors Veneto, Style Emme, Style Elle, ou Etrusco) appartient à la famille des revêtements linoléum en lés avec armature en toile de jute sur envers en mousse polyuréthane issue du recyclage. Il contient plus de 70% de matières premières naturelles (huile de lin, résine de pin, farine de liège et de bois, charge minérale, jute) et plus de 30% de matière recyclée. Le traitement de protection xf™2 appliqué en fin de fabrication évite le décapage et la métallisation pendant toute la durée de vie du produit, permettant ainsi sa mise en trafic immédiate après le nettoyage de fin de chantier. Les joints entre lés seront traités avec le cordon de soudure xf™2. Le taux d’émission de composés organiques volatils dans l'air de Linosom Silencio xf™2 est inférieur à 100 µg/m³ (COVT après 28 jours). Il possède une efficacité acoustique de 18 dB et un classement U4P3E1/2C2 sous Avis Technique. Linosom Silencio xf™2 bénéficie d'une Garantie 10 ans. Il est 100 % recyclable et bénéficie de la certification Cradle to Cradle® (niveau basic)." (IFCTEXT)
    Reference = "Linoleum_Veneto_Silencio_xf2_Apple Green_14892754" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Finition sol souple" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Description = "Le revêtement de sol sélectionné du type Linosom Silencio xf™2 (décors Veneto, Style Emme, Style Elle, ou Etrusco) appartient à la famille des revêtements linoléum en lés avec armature en toile de jute sur envers en mousse polyuréthane issue du recyclage. Il contient plus de 70% de matières premières naturelles (huile de lin, résine de pin, farine de liège et de bois, charge minérale, jute) et plus de 30% de matière recyclée. Le traitement de protection xf™2 appliqué en fin de fabrication évite le décapage et la métallisation pendant toute la durée de vie du produit, permettant ainsi sa mise en trafic immédiate après le nettoyage de fin de chantier. Les joints entre lés seront traités avec le cordon de soudure xf™2. Le taux d’émission de composés organiques volatils dans l'air de Linosom Silencio xf™2 est inférieur à 100 µg/m³ (COVT après 28 jours). Il possède une efficacité acoustique de 18 dB et un classement U4P3E1/2C2 sous Avis Technique. Linosom Silencio xf™2 bénéficie d'une Garantie 10 ans. Il est 100 % recyclable et bénéficie de la certification Cradle to Cradle® (niveau basic)." (IFCTEXT)
    Reference = "Linoleum_Veneto_Silencio_xf2_Carmine_14892645" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 3 more contents on 3 objects not shown
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 19.9999999999974 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Enrobé végétaux a froid" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Dalle en béton 20 + iso 10" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 19.9999999999968 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 20. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Aire de jeux sol souple ext" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Finition béton peinture lessivable" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Linoleum_Veneto_Silencio_xf2_Apple Green_14892754" (IFCIDENTIFIER)
  Pset_SlabCommon: 12 more contents on 12 objects not shown
  Pset_WindowCommon | properties | on 15 objects (15 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Chassis h1.60 x 240 aluminium 1 ouvrant OB et 2 fixes" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 12 objects (12 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "h160x240 Triple Vitrage- Store intérieur- 1 ouvrant OB et 2 fixes" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 10 objects (10 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "D 600 mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 6 objects (6 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "160x120 triple vitrage store interieur" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "160x240 Store Griesser aluminium 1 ouvrant OB et 2 fixes" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "chassis menuisé largeur 5.00x h 1.60" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "160x120 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0.45m x 0.45m - Appui Alu" (IFCIDENTIFIER)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Monobloc" (IFCIDENTIFIER)
    RiserHeight = 0.152490909090909 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.335018181818182 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Escalier technique" (IFCIDENTIFIER)
    RiserHeight = 0.171428571428589 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.257142857142823 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Profondeur de structure 80 mm" (IFCIDENTIFIER)
    RiserHeight = 0.152490909090909 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.335018181818182 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.335018181818182 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WaistThickness = 1.19999999999999 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 0.599999999999996 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Profondeur de structure 80 mm" (IFCIDENTIFIER)
    RiserHeight = 0.171428571428589 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.257142857142823 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.257142857142823 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WaistThickness = 0.9 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 0.45 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Construction | properties | on 27 objects (27 IFCCOLUMN)
    Extension inférieure = 0. (IFCLENGTHMEASURE) [METRE]
    Extension supérieure = 0. (IFCLENGTHMEASURE) [METRE]
    Style de coupe de base = "Horizontale" (IFCIDENTIFIER)
    Style de coupe supérieur = "Perpendiculaire" (IFCIDENTIFIER)
  Construction | properties | on 22 objects (22 IFCFURNISHINGELEMENT)
    Base = "Legs" (IFCLABEL)
    Cabinet Door = "Original" (IFCLABEL)
    Laminate Endplate Left = FALSE (IFCBOOLEAN)
    Laminate Endplate Right = FALSE (IFCBOOLEAN)
    Locking = "Klinka skola för hänglås a3906" (IFCLABEL)
  Construction | properties | on 3 objects (3 IFCCOLUMN)
    Décalage de l'attachement en haut = 0. (IFCLENGTHMEASURE) [METRE]
    Justification de l'attachement en haut = "Intersection minimale" (IFCIDENTIFIER)
  Construction | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Débuter avec contremarche = TRUE (IFCBOOLEAN)
    Etendre la base de contremarche inférieure = 0. (IFCLENGTHMEASURE) [METRE]
    Finir avec contremarche = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 object (1 IFCROOF)
    Coupe en chevron = "Coupe verticale" (IFCIDENTIFIER)
    Hauteur maximale de l'arrête = 159.272336038822 (IFCLENGTHMEASURE) [METRE]
    Profondeur du bord de toiture = 0. (IFCLENGTHMEASURE) [METRE]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Type de persienne = "Lames courbes" (IFCLABEL)
  Construction | properties | on 1 object (1 IFCROOF)
    Coupe en chevron = "Coupe verticale" (IFCIDENTIFIER)
    Hauteur maximale de l'arrête = 156.883842077225 (IFCLENGTHMEASURE) [METRE]
    Profondeur du bord de toiture = 0. (IFCLENGTHMEASURE) [METRE]
  Construction | properties | on 1 object (1 IFCROOF)
    Coupe en chevron = "Coupe verticale" (IFCIDENTIFIER)
    Hauteur maximale de l'arrête = 156.863667915155 (IFCLENGTHMEASURE) [METRE]
    Profondeur du bord de toiture = 0. (IFCLENGTHMEASURE) [METRE]
  Construction: 2 more contents on 2 objects not shown
  Pset_CoveringCommon | properties | on 11 objects (11 IFCCOVERING)
    Reference = "Faux plafond type ecophon hygiène 600x600" (IFCIDENTIFIER)
    TotalThickness = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    Reference = "Faux-Plafond Placostyl CF1/2h00" (IFCIDENTIFIER)
    TotalThickness = 0.025 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    Reference = "Faux-Plafond Placostyl CF1h00" (IFCIDENTIFIER)
    TotalThickness = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 266.611054000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
    TotalArea = 283.721557563172 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 172.899999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
    TotalArea = 183.996336861081 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 167.399003137124 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
    TotalArea = 178.142298273152 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.6226541953158 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
    TotalArea = 52.8073256059136 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 45.4117132024765 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "tuile terre cuite" (IFCIDENTIFIER)
    TotalArea = 48.3261358001263 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_ConcreteElementGeneral | properties | on 2 objects (2 IFCDOOR)
    FireRating = "PF 1/2H" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    FireRating = "Conformément à la réglementation en vigueur" (IFCLABEL)
  Visibilité | properties | on 4 objects (2 IFCDOOR, 2 IFCOPENINGELEMENT)
    vantail = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 20 objects (20 IFCBUILDINGELEMENTPROXY)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Reference = "E905601 - ULYSSE PACK SH DC AL LAT AVEC AB BLANC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Reference = "P504501 - ABATTANT UNIVERSEL K CHARN,INOX BLANC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Reference = "E903401 - ULYSSE RES,DC AL LAT BLANC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "Chitalpa Touffe 150" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "double porte 1500 x 1000" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Mûrier 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Brise soleil" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 3 more contents on 3 objects not shown
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "76X140" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 7.663 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "200 x 600 mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3.668 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "coupe feu" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 7.7 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "200 x 600 mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3.482 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "400 x 600 mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6.55 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "140 x 250" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5.618 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "140 x 250" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3.257 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "140 x 250" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3.84 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon: 13 more contents on 13 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 15 objects (15 IFCBEAM)
    Reference = "76X140" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 3 objects (3 IFCBEAM)
    Reference = "140 x 250" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM)
    Reference = "200 x 600 mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM)
    Reference = "coupe feu" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM)
    Reference = "400 x 600 mm" (IFCLABEL)
  Matériaux et finitions | properties | on 210 objects (210 IFCFURNISHINGELEMENT)
    Repose pieds = "Bois - Bouleau" (IFCLABEL)
  Matériaux et finitions | properties | on 34 objects (34 IFCCOLUMN)
    Matériau structurel = "Acier structurel - S235" (IFCLABEL)
  Matériaux et finitions | properties | on 18 objects (18 IFCBEAM)
    Matériau structurel = "Bois - Bois de construction de dimensions courantes" (IFCLABEL)
  Matériaux et finitions | properties | on 8 objects (8 IFCCOLUMN)
    Matériau structurel = "Bois - Pin" (IFCLABEL)
  Matériaux et finitions | properties | on 4 objects (4 IFCBEAM)
    Matériau structurel = "Béton - Béton coulé sur place" (IFCLABEL)
  Position géométrique | properties | on 7 objects (7 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Extension de départ = 0. (IFCLENGTHMEASURE) [METRE]
    Extension de fin = 0. (IFCLENGTHMEASURE) [METRE]
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Réduction du joint de début = -0.140020890880306 (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 2.94 (IFCLENGTHMEASURE) [METRE]
  Position géométrique | properties | on 3 objects (3 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 3.6 (IFCLENGTHMEASURE) [METRE]
  Position géométrique | properties | on 3 objects (3 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Extension de départ = 0. (IFCLENGTHMEASURE) [METRE]
    Extension de fin = 0. (IFCLENGTHMEASURE) [METRE]
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 2.94 (IFCLENGTHMEASURE) [METRE]
  Position géométrique | properties | on 1 object (1 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 3.35 (IFCLENGTHMEASURE) [METRE]
  Position géométrique | properties | on 1 object (1 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Extension de départ = 0. (IFCLENGTHMEASURE) [METRE]
    Extension de fin = 0. (IFCLENGTHMEASURE) [METRE]
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Réduction du joint d'extrémité = -0.192875152010526 (IFCLENGTHMEASURE) [METRE]
    Réduction du joint de début = -0.0985979040629636 (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 2.8 (IFCLENGTHMEASURE) [METRE]
  Position géométrique | properties | on 1 object (1 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Extension de départ = -0.192875152010531 (IFCLENGTHMEASURE) [METRE]
    Extension de fin = 0. (IFCLENGTHMEASURE) [METRE]
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Réduction du joint de début = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 2.8 (IFCLENGTHMEASURE) [METRE]
  Position géométrique | properties | on 1 object (1 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Extension de départ = -0.150379507974969 (IFCLENGTHMEASURE) [METRE]
    Extension de fin = 0. (IFCLENGTHMEASURE) [METRE]
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Réduction du joint de début = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 2.8 (IFCLENGTHMEASURE) [METRE]
  Position géométrique | properties | on 1 object (1 IFCBEAM)
    Etat de la jonction = "Deux jonctions activées" (IFCIDENTIFIER)
    Extension de départ = 0. (IFCLENGTHMEASURE) [METRE]
    Extension de fin = 0. (IFCLENGTHMEASURE) [METRE]
    Justification Y = "Origine" (IFCIDENTIFIER)
    Justification YZ = "Uniforme" (IFCIDENTIFIER)
    Justification Z = "Haut" (IFCIDENTIFIER)
    Réduction du joint de début = -0.140926173371718 (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Y = 0. (IFCLENGTHMEASURE) [METRE]
    Valeur de décalage Z = 2.94 (IFCLENGTHMEASURE) [METRE]
  Position géométrique: 4 more contents on 4 objects not shown
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Facade panneau simple" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 10 objects (10 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Vitré" (IFCIDENTIFIER)
    ThermalTransmittance = 6.7069 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_MemberCommon | properties | on 3 objects (3 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 2.20656854249491 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 0.681819805153406 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 1.58635522160779 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 1.37718578426459 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 1.99483967674094 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 1.23661980515339 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 2.61040355972863 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "100 x 10 mm metal incliné" (IFCIDENTIFIER)
    Span = 1.98 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon: 4 more contents on 4 objects not shown
  Quadrillage horizontal | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Décaler = 0. (IFCLENGTHMEASURE) [METRE]
    Justification = "Début" (IFCIDENTIFIER)
    Nombre = 4 (IFCINTEGER)
  Quadrillage vertical | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Décaler = 0. (IFCLENGTHMEASURE) [METRE]
    Justification = "Début" (IFCIDENTIFIER)
    Nombre = 4 (IFCINTEGER)
  Electricité - Charges | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Numéro de circuit = "" (IFCTEXT)
    Panneau = "" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 10 objects (10 IFCFLOWTERMINAL)
    Reference = "1000mm x 462mm" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 9 objects (9 IFCFLOWTERMINAL)
    Reference = "Lave main cuisine" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Reference = "Urinoir" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 34 objects (34 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RO168.3x3" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "300x300mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ReinforcementBarPitchOfColumn | properties | on 34 objects (34 IFCCOLUMN)
    Reference = "RO168.3x3" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 8 objects (8 IFCCOLUMN)
    Reference = "300x300mm" (IFCLABEL)
  Génie climatique | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Abréviation du système = "" (IFCTEXT)
    Classification du système = "Eau froide sanitaire,Sanitaire" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Génie climatique | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Abréviation du système = "" (IFCTEXT)
    Classification du système = "Eau froide sanitaire" (IFCTEXT)
    Nom du système = "" (IFCTEXT)

Other addresses and roles
  postal address: "Boulevard des Campanhols Castanet-Tolosan 31320", "Romainville", "Seine-St.-Denis", "France"